**New Product Release – March 2022**

ISLG **Overhaul Kit**

New engine overhaul kit **MCB5633416** is now available for Cummins® ISLG 8.9L CM2180 engine applications. The upper gasket set included in this new kit contains the updated head gasket along with high temperature seals. This engine kit also contains piston kit **M-5406084** which features a forged steel crown and skirt with graphite skirt coating for improved scuff resistance. Additionally, the piston kit contains new piston cooling jets. Contact Interstate-McBee for more details.

|  |
| --- |
| Kit - Piston |
| Kit - Engine Overhaul |
| Nozzle - Piston Cooling |

**Overhaul Kits Include:**

Piston Kits

Piston Rings

Piston Cooling Nozzles

Liner Kits

Main Bearings

Connecting Rod Bearings

Lower Gasket Set

Upper Gasket Set

ISX/QSX **Fuel Pump Repair Kits**

Interstate-McBee offers popular fuel pump repair kits for Cummins® ISX/QSX - HPI applications. Kits **M-4089431RK** and **M-4089431RKS** can be used to service the 4089431 and 4089163 fuel pumps. These kits contain high temperature molded seals, a replacement main shaft, a hardened hexagonal drive shaft, and a premium double drive shaft seal kit with installer. The **M-4084931RKS** kit also contains the additional seals and gaskets used to reseal the damper (buffer). Using our service kits can save hundreds when compared with buying a replacement pump assembly.

Fuel pump gasket **M-4954471** is also available to service early style gear pumps.

|  |  |
| --- | --- |
| **Part Number** | **Description** |
| M-4089431RK | Repair Kit - Fuel Pump |
| M-4089431RKS | Repair Kit - Fuel Pump |

ISB6.7L **Piston and Overhaul Kits**

Interstate-McBee is expanding its coverage of popular Cummins ISB6.7L engines. New piston kits and engine kits are now available for later model 6.7L HPCR engines popular in both industrial and pickup truck applications. The piston kits are used in HPCR CM2150, CM2250, and CM2350 engine applications and feature gallery cooling to help lower piston crown and ring pack temperatures. The new pistons also incorporate graphite skirt coating to improve scuff resistance in these highly loaded applications. The **M-PK5336102** and **M-4376348** pistons are .50mm oversize for servicing a worn cylinder block. These new pistons are offered in many different Inframe and Overhaul kits so please contact Interstate-McBee for more details and exact applications.

|  |
| --- |
| Kit - Piston Std. |
| Kit - Piston .50mm |
| Kit - Inframe |
| Kit - Overhaul |
| Pickup Trucks |
| Industrial |

**Kits Include:**

|  |  |  |
| --- | --- | --- |
| **Piston Kit** | **Inframe Kit** | **Overhaul Kit** |

|  |
| --- |
| **Piston** |
| **Piston Rings** |
| **Piston Pin Retainers** |
| **Main Bearings** |
| **Connecting Rod Bearings** |
| **Lower Gasket Set** |
| **Oil Pan Gasket** |
| **Flange Gasket** |
| **Upper Gasket Set** |